**C-shield parylene allows major weight saving for EM shielding of microelectronics**

**Published in:**[Proceedings. The First IEEE International Symposium on Polymeric Electronics Packaging, PEP '97 (Cat. No.97TH8268)](https://ieeexplore.ieee.org/xpl/conhome/5267/proceeding)

